**UBS-5324z**

24 port RJ-45 10/100/1000Mbps 工程用網管交換器

26.7公分小台，弱電箱體可放，有壁掛孔

符合台灣安規BSMI

施工簡單，附19”機架腳架，可以安裝在標準機櫃

|  |  |
| --- | --- |
| 24 port RJ-45 10/100/1000Mbps網管交換器  支援 MDI/MDI-X 自動跳線  支援 NWay protocol and auto-detection  相容IEEE802.3, 802.3u, 802.3ab Ethernet standards  支援 IEEE802.3x Flow Control and Back-Pressure control  支援 STP & RSTP (防Loop功能)  支援 LLDP Discovery  支援 VLAN : Static, Group, Tag Based, Voice OUI mode  支援 QoS : Priority Queue, Rate Limit, Queue Scheduling, Class of Service  支援 Security : Storm Control, HTTPS and SSL 2.0, Account Manager, Management VLAN, DoS attack prevention  支援 IPv6 : IPv6 Host and IPv6 Application  支援 Management : CLI (Console, Telnet), Web UI (HTTP and HTTPS), SNMP v1/v2c, MIBs (MIBII & RMON I(1,2,3,9 groups))  支援 Storm Filter (Broadcast, Unknown Multicast, Unknown Unicast)  支援 8 queues is handled SP and WRR  支援 Jumbo Frame : 1518~10K Bytes  支援 8 Link Aggregation Groups with Static & LACP types  支援 port mirroring鏡像 , Copper Testing  支援 IGMP Snooping v2/v3  支援 IEEE802.3az EEE enable and disable  支援韌體更新和備份功能  支援設定檔備份和還原功能 | **Standard**  IEEE802.3, IEEE802.3u, IEEE802.3ab, IEEE802.3x, IEEE802.3az, IEEE 802.1p standards  **Interface**  24 \* 10/100/1000Mbps RJ-45 NWay ports  1 \* Power on/off switch  1 \* Reset to default setting button  **Rich LED indicators**  Power (Green)  System (Green)  Per Port: Link/Act(Green)  **MAC Address Table**  8K  **Jumbo Frame**  10K Bytes  **Buffer Memory**  524.8K Bytes  **Emission & Safety 認證安規**  BSMI  **Operating Temperature(操作溫度)**  0度c- 50度c (32度F- 122度F)  Operating Humidity  10% ~ 90% RH(non-condensing)  **Dimension(體積大小)**  267x 162x 42mm  **Power Supply**  100~240VAC input, 50/60Hz. |

**UBLink.org**